# Mnemonics

'PS' | Auxiliary Port On

Character Printer

## Description

'PS' contains the auxiliary port on sequence that tells the terminal to route incoming characters to the auxiliary port instead of the terminal's display area.

This sequence remains active until an off sequence is encountered via the 'PE' mnemonic. This should be defined in the device driver for the terminal type and then retrieved and set on the printer channel.

## See Also

'PE' Auxiliary Port Off