# System Parameters

'00' | Don't Display NULL Bytes

## Description

The '00' parameter is used to control the transmission of $00$ to terminal and/or window screen devices. Some devices ignore the transmission of $00$, whereas, by default, Windows screens consider $00$ to be a character for the purposes of display.

Setting this parameter forces the system to strip any $00$ bytes from a PRINT string.

(The '00' system parameter was added in PxPlus v8.11, build 9182.9.)

## Default

Off - which means NULL bytes will be sent.